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	 (Product Code)：CB15500310
Model 

KFRI25GN
Function 

COOLING

HEATING

Rated Voltage 

220-240V～
Frequency(Hz)

80/50/25

80/53/25

Total Capacity (W) (High/Standard/Low *):

Total Capacity (Btu/h) (High/ Standard/Low *):

3100/2500/1180
10600/9000/4036
3800/2750//1200
13000/9386/4096
Power Input (W) (High/ Standard/Low *)
1330/730/280
1365/745/310
Rated Input (W)

1400
1450
Rated Current (A)

6.1
6.3
Air Flow Volume (m3/h) 

500
Dehumidifying Volume (l/h)

1.2
EER / C.O.P (W/W) 
 2.33/3.42/4.21
2.784/3.69/3.87
Energy Class

A/A
Indoor  unit
Model of Indoor Unit

KFRI25GN
Fan Motor Speed (r/min) (H/M/L)

Cooling:(1260)/1050/920/730

Heating:(1320)/1200/1100/950
Output of Fan Motor (w)

10
Input Power of  Heater  (w)

None

Fan Motor Capacitor (uF)

1.0
Fan Motor RLA(A)

0.1
Fan Type-Piece

Cross flow fan – 1

Diameter-Length (mm)

φ85×596
Evaporator

Aluminum fin-copper tube
Pipe Diameter (mm)

Φ7

Row-Fin Gap(mm) 
2-1.5

Coil length (l) x height (H) x coil width (L)

581X264X25.4

Swing Motor Model

MP24AA

Output of Swing Motor (W)

1.5

Fuse (A)

PCB 3.15A   
Sound Pressure Level dB (A) (H/M/L)

(40)/37/31/23

Sound Power Level dB (A) (H/M/L)***

(50)/47/41/33①
Dimension (W/H/D) ( mm)
790×265×170
Dimension of Package (L/W/H)( mm)

870×248×355
Net Weight /Gross Weight (kg)

9 / 12

Note：

1．Test  Standard：

2．*Inverter different Compressor speed
3．** Fan different speed
4．*** Approximate Calculation from Sound Pressure Level to Sound Power Level:

Average Sound Pressure Level
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：Sound pressure level of front test point
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：Sound pressure level of side test point，for indoor unit 
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Approximate Sound Power Lever
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	Outdoor unit
Model of Outdoor Unit

KORI25GN
Compressor Manufacturer/trademark 

MITSUBISHI

Compressor Model

KNB092FHBMC

Compressor Type

single-rotor
L.R.A. (A)

25
Compressor RLA(A)

3.89

Compressor Power Input(W)

895

Overload Protector

None

Throttling Method

Capillary throttling

Starting Method

Transducer starting

Working Temp Range (℃)

-15℃≤T≤43℃
Condenser 

Aluminum fin-copper tube 

Pipe Diameter (mm)

9.52

Rows-Fin Gap(mm)

1-1.6

Coil length (l) x height (H) x coil width (L)

608X508X22

Fan Motor Speed (rpm) (H/M/L)

830±20

Output of Fan Motor (W)

30

Fan Motor RLA(A)

0.3

Fan Motor Capacitor (uF)

2.5

Air Flow Volume of Outdoor Unit

/

Fan Type-Piece

Axial fan –1

Fan Diameter (mm)

400

Defrosting Method

Auto defrost

Climate Type

T1

Isolation

I

Moisture Protection

IP24

Permissible Excessive Operating Pressure for the Discharge Side(MPa)

3.8

Permissible Excessive Operating Pressure for the Suction Side(MPa)

1.2

Sound Pressure Level dB (A) (H/M/L)

53   

Sound Power Level dB (A) (H/M/L)

63   

Dimension (W/H/D) ( mm)

848X260X540

Dimension of Package (L/W/H)( mm)

878X360X580
Net Weight /Gross Weight (kg)

35/40

Refrigerant and Charge (kg)

R410A / 0.8
Connection Pipe

Length (m)

4

Gas additional charge(g/m)

15

Outer Diameter 

Liquid Pipe (mm)

Φ6(1/4”)

Gas Pipe (mm)

Φ9.52(3/8”)

Max Distance

Height (m)

5

Length (m)

10

Loading Quantity

20’ Container

Interior Dimensions L*W*H：5898*2352*2393，Door Opening W*H：2343*2280

90

40’ Container

Interior Dimensions L*W*H：12032*2350*2390，Door Opening W*H：2343*2280

188

40’ High Cube Container

Interior Dimensions L*W*H：12032*2350*2697，Door Opening W*H：2338*2585

212
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