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	 (Product Code)：CB15500030

Model 

KFRI50GN-KORI50GN
Function 

COOLING

HEATING

Rated Voltage 

220-240V~

Frequency(Hz)

50Hz

Total Capacity (W) Standard (Low~High):

Total Capacity (Btu/h) Standard (Low~High):

5275（1260~6600）

18000（4300~22500）

5850（1120~6800）

20000（3800~23200）

Power Input (W) Standard (Low~High):

1600（380~2650）

1620（350~2650）

Rated Input (W)

2650
2650

Rated Current (A)

12.0

12.0

Air Flow Volume (m3/h) (SH/H/M/L)
850/780/650/550

Dehumidifying Volume (l/h)

2.0

EER / C.O.P (W/W) 

3.30

3.61

Energy Class

A

A

Indoor  unit

Model of Indoor Unit

KFRI50GN
Fan Motor Speed (r/min) (H/M/L)

1350/1200/1050/900

1420/1250/1150/1050

Output of Fan Motor (w)

20

Input Power of Heater (w)

/

Fan Motor Capacitor (uF)

1.5

Fan Motor RLA(A)

0.25

Fan Type-Piece

Cross flow fan – 1

Diameter-Length (mm)

Φ98X710

Evaporator

Aluminum fin-copper tube

Pipe Diameter (mm)

Φ7

Row-Fin Gap(mm) 

2-1.4

Coil length (l) x height (H) x coil width (L)

715X304.8X25.4

Swing Motor Model

MP28VB

Output of Swing Motor (W)

2.5

Fuse (A)

PCB 3.15A   Transformer 0.2A

Sound Pressure Level dB (A) (H/M/L)

46/44/40/35

Sound Power Level dB (A) (H/M/L)***

56/54/50/45

Dimension (W/H/D) ( mm)

940X298X200

Dimension of Package (L/W/H)( mm)

1010X285X380

Net Weight /Gross Weight (kg)

13/17

Note：

1．Test  Standard：

2．*Inverter different Compressor speed

3．** Fan different speed
4．*** Approximate Calculation from Sound Pressure Level to Sound Power Level:

Average Sound Pressure Level
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：Sound pressure level of front test point


[image: image4.wmf]2

P

L


：Sound pressure level of side test point，for indoor unit 
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Approximate Sound Power Lever
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	Outdoor unit
Model of Outdoor Unit

KORI50GN
Compressor Manufacturer/trademark 

China Resources (Shenyang) Sanyo CO.,LTD

Compressor Model

C-6RZ146H1A
Compressor Type

Twin rotary compressor

L.R.A. (A)

41

Compressor RLA(A)

8.4

Compressor Power Input(W)

1640

Overload Protector

1NT11L-3979
Throttling Method

Electric expand valve

Starting Method

Transducer starting

Working Temp Range (℃)

5℃≤T≤46℃
-15℃≤T≤30℃
Condenser 

Aluminum fin-copper tube

Pipe Diameter (mm)

7

Rows-Fin Gap(mm)

1-1.4
Coil length (l) x height (H) x coil width (L)

870x660x19.05

Fan Motor Speed (rpm) (H/M/L)

690/500
Output of Fan Motor (W)

60W
Fan Motor RLA(A)

0.62
Fan Motor Capacitor (uF)

3
Air Flow Volume of Outdoor Unit（m3/h）

2700
Fan Type-Piece

Axial fan –1
Fan Diameter (mm)

Φ520
Defrosting Method

Auto defrost
Climate Type

T1

Isolation

I

Moisture Protection

IP24

Permissible Excessive Operating Pressure for the Discharge Side(MPa)

3.8
Permissible Excessive Operating Pressure for the Suction Side(MPa)

1.2
Sound Pressure Level dB (A)

54
Sound Power Level dB (A)

64
Dimension (W/H/D) ( mm)

890X700X340
Dimension of Package (L/W/H)( mm)

1030X460X735
Net Weight /Gross Weight (kg)

47/52
Refrigerant and Charge (kg)

R410A/1.10
Connection Pipe

Length (m)

5

Gas additional charge(g/m)

50

Outer Diameter 

Liquid Pipe (mm)

Φ6

Gas Pipe (mm)

Φ12

Max Distance

Height (m)

10

Length (m)

30

Loading Quantity

20’ Container

Interior Dimensions L*W*H：5898*2352*2393，Door Opening W*H：2343*2280

60

40’ Container

Interior Dimensions L*W*H：12032*2350*2390，Door Opening W*H：2343*2280

127

40’ High Cube Container

Interior Dimensions L*W*H：12032*2350*2697，Door Opening W*H：2338*2585

147
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